Steps for enrolling a 5834 Wireless Key Transmitter

***Take Keyfob out of high security mode (You need a green light NOT a red light on the keyfob)***

 Hold “Disarm” “Aux” and “Arm Stay” (all three buttons at the same time) for about 5 seconds.

 Release the buttons and hold the disarm button; if the LED light blinks green on the keyfob you

have the correct setting. If it is red, try again.

***Programming***

 Type in your installer code, followed by 800 (Default is 4112+800)

 Press \*56 (Zone Programming)

 Push 1 for yes to SET to Confirm

 Keyfobs should start on zone 49, so type 4 then 9

 Hit \* to skip summary screen

 Hit \* to get to zone type screen.

 For each button you will have to create a new zone. Below are the 4 types typically used for a 4

button transmitter. For Zone 49 select 2 then 1 for Arm Away.

 21 = Arm Away (Top Left Button)

 22 = Disarm (Top Right Button)

 20 = Arm Stay (Bottom Left Button)

 07 = Police Panic (Bottom Right Button)

 Hit \* to confirm

 Press 1 for partition 1

 Hit \* to continue to report code screen

 Hit \* to continue to input type screen

 Push 5 and you should see “BUTTON RF”

 Push \* to continue to Serial Number Screen

 Hold down the correct button on the keyfob you want to assign to the particular zone type until

 The system beeps and the serial number appears on the screen. Wait a few seconds and hold it

down again until it beeps again.

 Hit \* to continue

 Wait 10 seconds and press and hold the button again to confirm the serial and loop numbers.

 Hit \* to confirm summary screen (49 21 1 10 BR:3s Should be close to what you have on your

screen at this point)

 Hit 0 to not program Alpha

 Continue programming as described for each of the buttons on the Keyfob according to the zon types listed above.

 When all buttons have been programmed type 00 to quit zone programming, then type \*99 to

exit installer programming.

The keyfob needs to be assigned a keypad code to function properly. To do this enter your 4

digit MASTER code (default is 1234) followed by 810#449 (this is user 10 and zone 49 keyfob) This should assign all of the 4 buttons on that keyfob to a user code and the keyfob should start to work.

For additional keyfobs repeat the process starting at zone 53, and assign a user code at the end

in the same fashion except for the next keyfob you would type MASTER code then 811#453 (User 11 and zone 53).